## Mirrors

#### Mirror Holder Replacement

20-171

1. Pry the mirror holder (A) out from the top, and detach the pivot (B).

Carefully move the mirror holder until you can see the joint pins (C), then release the retainer springs (D) using a flat tip screwdriver.

2. Detach the joint pins (A) from the mirror holder (B), then remove the mirror holder.

3. If equipped, disconnect the mirror defogger connector.

4. Install the mirror holder in the reverse order of removal, and note these items:

- Before installing the mirror holder (A), install the retainer spring (B) on the mirror holder.
- If equipped, make sure the mirror defogger connector is plugged in properly.
- Grease the pivot (C) and joint pins (D).
- Reattach the mirror holder (A) to the pivot and joint pin of the actuator, then carefully push the pivot and joint pin portions of the mirror holder until the mirror holder locks into place.
- Check the operation of the actuator.