## Hood

#### Adjustment (cont'd)

20-107

Hood Seal Replacement

4. Check that the hood opens properly and locks securely.

5. Apply touch-up paint to the hinge mounting bolts and around the hinges.
6. Grease each location of the hood latch and hood hinge as indicated by the arrows.

1. Using a clip remover, detach the clips (A, B), then remove the hood seal (C) and hood sub-seal (D). Take care not to scratch the hood.

Fastener Locations
A : Clip, 14 | B : Clip, 2

2. Install the seals in the reverse order of removal, and replace any damaged clips.