## Honda Multi Matic Transmission/CVT

#### Transmission Removal (cont'd)

14-329

30. Remove the transmission housing mounting bolts.

31. Place a jack under the transmission.
32. Remove the transmission mount bracket.

33. Remove the transmission housing mounting bolt (A), rear mount bracket bolts (B) and rear mount/bracket (C).

34. Pull the transmission away from the engine until it clears the dowel pins, then lower it on the jack.
35. Remove the flywheel (A) and starter (B) from the transmission.