## Rear Suspension

#### Hub Bearing Unit Replacement – Drum Brake

18-24

Exploded View

4-door

1. SPINDLE

   Check for bend and deformation.

2. BRAKE DRUM

   Check for wear and damage.

3. SPINDLE NUT

   22 x 1.5 mm, 181 Nm (18.5 kgf/m, 134 lbf/ft), Replace.

4. HUB CAP, Replace.
5. HUB BEARING UNIT

   Check for faulty movement and wear.

6. REAR BRAKE ASSY

5-door:

1. SPINDLE

   Check for bend and deformation.

2. BRAKE DRUM

   Check for wear and damage.

3. SPINDLE NUT

   22 x 1.5 mm, 181 N m (18.5 kgf/m 134 lbf/ft), Replace.

4. HUB CAP, Replace.
5. HUB BEARING UNIT

   Check for faulty movement and wear.

6. REAR BRAKE ASSY