## Manual Transmission

#### Transmission Disassembly

13-15

Exploded View-Clutch Housing

1 2 3 4 5

6

7

8

9

INPUT SHAFT ASSEMBLY

OUTPUT SHAFT ASSEMBLY

REVERSE DETENT PLUG, REVERSE DETENT SPRING AND REVERSE DETENT BALL

25 Nm (2.5 kgf/m, 18 lbf/ft)

TRANSMISSION CASE DOWEL PIN

INTERLOCK PIN

TRANSMISSION CABLE LOWER BRACKET

8 x 1.25 mm FLANGE BOLT

25 Nm (2.5 kgf/m, 18 lbf/ft)

TRANSMISSION CASE UPPER BRACKET

8 x 1.25 mm FLANGE BOLT

25 Nm (2.5 kgf/m, 18 lbf/ft)

10

11

12

13

14

15

16

17

18

19

20

21

22

CABLE CLIP BRACKET

SPEEDOMETER DRIVEN GEAR

6 x 1.0 mm RETAINER BOLT

6 Nm (0.6 kgf/m, 52 lbf/ft)

SPEED SENSOR RETAINER

CLUTCH HOUSING

TRANSMISSION CASE MAGNET

REVERSE SHIFT LEVER

DIFFERENTIAL GEAR ASSEMBLY

FRT OUTPUT SHAFT OIL NOZZLE

1ST/2ND, 3RD/4TH SHIFT ROD AND ARM ASSEMBLY

5TH SHIFT ARM

SHIFT ARM SPRING PIN

5TH/REVERSE SHIFT ROD AND BLOCK ASSEMBLY

23

24

25

26

27

28

29

30

31

32

SLAVE CYLINDER BRACKET

8 x 1.25 mm FLANGE BOLT

25 Nm (2.5 kgf/m, 18 lbf/ft)

REVERSE LEVER FULCRUM BRACKET

8 x 1.25 mm FULCRUM BRACKET BOLT

19 Nm (1.9 kgf/m, 14 lbf/ft)

BEARING RING

REVERSE IDLER GEAR, REVERSE IDLER SHAFT AND REVERSE IDLER SHAFT STRAIGHT PIN

WASHER

10 x 1.25 mm REVERSE IDLER SHAFT BOLT

38 Nm (3.8 kgf/m, 28 lbf/ft)

STRAIGHT KNOCK PIN

INPUT SHAFT OIL SEAL

a a a