## Seats

#### Rear Seat-back Cover Replacement – Folding Type

20-99

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.

1. Remove the seat-back (see page 20-95), and if equipped, remove the headrest.
2. On the left seat-back for some models: Remove the screw, then remove the centre belt guide (A).

   Fastener Location
   : Screw, 1

3. Release the hook (A), and unzip the seat-back cover (B). The left seat-back is shown, the right seat-back is similar.

4. Pull back the seat-back cover (A), and remove the clips (B), and release the hooks (C).

Fastener Location
B : Clip | Left, 6
| Right, 3

Left seat back:

Right seat back: