## Exterior Trim

#### Front Grille Replacement

20-113

Hood Moulding Replacement

1. Remove the front bumper (see page 20-104).

2. Remove the screws (A) and clips (B), and remove the front grille (C) from the front bumper (D) by pulling it out. Take care not to scratch the front bumper.

   Fastener Locations
   A : Screw, 2 | B : Clip, 4

3. Remove the screws, then remove the front grille cover (A) from the front grille (B).

   Fastener Locations
   : Screw, 6

4. Install the grille in the reverse order of removal, and replace any damaged clips.

1. Remove the nuts (A), and detach the clip (B) by pushing it from the drain hole (C) in the hood, then remove the hood moulding (D). Take care not to scratch the hood.M

Fastener Locations
A : Nut, 4 | B : Clip, 1

2. Install the moulding in the reverse order of removal, and replace the clip if it's damaged.