## Plastic Parts Paint

#### Features of Plastic Material

6-11

- Check each of the plastic parts for solvent resistance and heat resistance temperatures before you do any repair work.
- Select the repair material according to materials of the plastic parts.

  Standard Symbol | Name | Heat Resistance Temperature °C (°F) | Solvent Resistance | Note
  AAS | Acrylonitrile acrylic styrene | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | An organic solvent such as gasoline is not recommended. An aroma product is not recommended.
  ABS | Acrylonitrile butadiene styrene | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | An organic solvent such as gasoline is not recommended. An aroma product is not recommended.
  AES | Acrylonitrile ethylene styrene | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | An organic solvent such as gasoline is not recommended. An aroma product is not recommended.
  A/EPDM/S | Acrylonitrile / ethylene propylene diene rubber / styrene | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | An organic solvent such as gasoline is not recommended. An aroma product is not recommended.
  ASA | Acrylonitrile styrene acrylate | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | An organic solvent such as gasoline is not recommended. An aroma product is not recommended.
  CAB | Cellulose acetate butylate | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | An organic solvent such as gasoline is not recommended. An aroma product is not recommended.
  E/VAC | Ethylene-vinyl acetate | 80 (176) | A small amount of alcohol and gasoline are acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended.
  PA | Polyamide | 80 (176) | Alcohol and gasoline are acceptable. | Battery acid (sulphuric acid) is not recommended.
  PBT | Polybutylene terephtalate | 160 (320) | Alcohol and gasoline are acceptable. | Solvent is not recommended.
  PC | Polycarbonate plastics | 120 (248) | A small amount of alcohol is acceptable for a short time. | Brake fluid, and wax and grease remover not recommended.
  PE | Polyethylene | 80 (176) | Alcohol and gasoline are acceptable. | Solvent is not recommended.
  PF | Phenol formaldehyde | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol, is not recommended.
  PMMA | Polymethyl methacrylate | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol, is not recommended. Wash remover off with water thoroughly.
  POM | Polyoxymethylene polyacetal | 100 (212) | Alcohol and gasoline are acceptable. | Solvent is not recommended.