## Clutch

#### Clutch Master Cylinder Replacement (cont'd)

12-6

1. Install the clutch master cylinder in the reverse order of removal. Install a new O-ring. Tighten the master cylinder mounting nuts to 13 Nm (1.3 kgf/m, 9.4 lbf/ft). Make sure the tabs on the master cylinder hose clamps are pointed in the directions shown.

1. To prevent the retaining clip (A) from coming off, pry open the tip of the retaining clip (B) with a screwdriver.

1. Bleed the clutch hydraulic system (see step 6 on page 12-9).

   NOTE: The reservoir filling is covered in the bleeding procedure.

a a a