## Engine Assembly

#### Engine Installation (cont'd)

5-14

20. Connect the upper radiator hose (A), lower radiator hose (B), heater hose (C) and ground cable (D).

21. Install the A/C compressor (A), then install the alternator lower bracket (B).

22. Install the A/C hose bracket (A) and P/S hose bracket (B).

23. Loosely install the alternator.
24. Adjust the alternator belt tension, refer to the '01 Civic Shop Manual on this CD (see page 4-38) or the alternator-compressor belt tension, refer to the '01 Civic Shop Manual on this CD (see page 4-37).
25. Loosely install the P/S pump belt and pump.
26. Adjust the P/S pump belt, refer to the '01 Civic Shop Manual on this CD (see page 17-23).
27. Push the ECM/PCM connectors through the bulkhead, then install the grommet (A).

28. Install the harness clamps (B).