## Power Steering

#### Steering Gearbox Installation (cont'd)

17-60

20. Install the front wheels.

21. Fill the system with power steering fluid, and bleed air from the system (see page 17-25).
22. After installation, perform the following checks.

- Start the engine, allow it to idle, and turn the steering wheel from lock-to-lock several times to warm up the fluid. Check the gearbox for leaks (see page 17-22).
- Perform the front toe inspection (see page 18-7).
- Check the steering wheel spoke angle. Adjust by turning the right and left tie-rods equally, if necessary.