## Standards and Service Limits

#### Honda Multi Matic Transmission and HMM Differential (cont'd)

2-20

Item | Measurement | Qualification | Standard or New | Service Limit
Clutch | Clutch end plate-to-top disc clearance | Forward clutch | 0.6-0.8 mm (0.024-0.031 in.) | -
Start clutch | 0.5-0.7 mm (0.020-0.028 in.) | -
Reverse brake | 0.45-0.75 mm (0.018-0.030 in.) | -
Clutch return spring free length | Forward clutch | 30.5 mm (1.20 in.) | 28.5 mm (1.12 in.)
Start clutch | 40.9 mm (1.61 in.) | 38.9 mm (1.53 in.)
Reverse brake | 29.4 mm (1.16 in.) | 27.4 mm (1.08 in.)
Clutch disc thickness | Forward clutch | 1.94 mm (0.076 in.) | -
Start clutch | 1.94 mm (0.076 in.) | -
Reverse brake | 2.00 mm (0.079 in.) | -
Clutch plate thickness | Forward clutch | 2.00 mm (0.079 in.) | When discoloured
Start clutch | 2.3 mm (0.091 in.) | When discoloured
Reverse brake | 1.35 mm (0.053 in.) | When discoloured
Forward clutch end plate | Mark 14 | 3.4 mm (0.134 in.) | When discoloured
Mark 15 | 3.5 mm (0.138 in.) | When discoloured
Mark 16 | 3.6 mm (0.142 in.) | When discoloured
Mark 17 | 3.7 mm (0.146 in.) | When discoloured
Mark 18 | 3.8 mm (0.150 in.) | When discoloured
Mark 19 | 3.9 mm (0.154 in.) | When discoloured
Mark 20 | 4.0 mm (0.157 in.) | When discoloured
Mark 21 | 4.1 mm (0.161 in.) | When discoloured
Mark 22 | 4.2 mm (0.165 in.) | When discoloured
Mark 23 | 4.3 mm (0.169 in.) | When discoloured
Mark 24 | 4.4 mm (0.173 in.) | When discoloured
Mark 25 | 4.5 mm (0.177 in.) | When discoloured
Mark 26 | 4.6 mm (0.181 in.) | When discoloured
Mark 27 | 4.7 mm (0.185 in.) | When discoloured
Reverse brake end plate | Mark 1 | 3.6 mm (0.142 in.) | When discoloured
Mark 2 | 3.8 mm (0.150 in.) | When discoloured
Mark 3 | 4.0 mm (0.157 in.) | When discoloured
Mark 4 | 4.2 mm (0.165 in.) | When discoloured
Mark 5 | 4.4 mm (0.173 in.) | When discoloured
Mark 6 | 4.6 mm (0.181 in.) | When discoloured
Mark 7 | 4.8 mm (0.189 in.) | When discoloured
Mark 8 | 5.0 mm (0.197 in.) | When discoloured