## Manual Transmission

#### Mainshaft Reassembly (cont'd)

13-32

1. Install the synchro spring (A).

1. Install the double cone synchro assembly (B) by aligning the synchro cone fingers (C) with the grooves in 3rd/4th synchro hub (D).

1. Install the 4th gear (A) by aligning the synchro cone fingers (B) with holes in 4th gear (C).

1. Install the needle bearings, distance collar, and 5th gear.

1. Install the double cone synchro assembly (A) by aligning the synchro cone fingers (B) with the holes in 5th gear (C), then install the synchro spring (D).

1. Install the 5th/6th synchro hub (A) by aligning the synchro cone fingers (B) with the grooves in 5th/6th synchro hub (C).

a a a