## Driveline/Axle

#### Intermediate Shaft Reassembly

16-21

Exploded View

1. INTERMEDIATE SHAFT RING
2. BEARING SUPPORT RING
3. FLANGE BOLT

   10 x 1.25 mm

   3.9 Nm (4.0 kgf/m, 29 lbf/ft)

4. DOWEL BOLTS

   10 x 1.25 mm

   39 Nm (4.0 kgf/m, 29 lbf/ft)

5. EXTERNAL SNAP RING
6. OUTER SEAL, Replace.
7. SET RING, Replace.
8. Pack the interior of the outer seal.
9. BEARING SUPPORT
10. INTERMEDIATE SHAFT BEARING, Replace.
11. INTERNAL SNAP RING
12. INTERMEDIATE SHAFT

a a a