## Clutch

#### Slave Cylinder Replacement

12-8

NOTE: Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.

1. Remove the mounting bolts (A) and the slave cylinder (B).

2. Remove the roll pins (C). Disconnect the clutch line (D) and remove the O-ring (E). Plug the end of the clutch line with a shop towel to prevent brake fluid coming out.

3. Install the slave cylinder in the reverse order of removal. Install the new O-ring (A).

4. Pull the boot (B) back and apply grease to the boot and slave cylinder rod (C). Reinstall the boot.

5. Apply Urea Grease UM264 (P/N 41211-PY5-305) to the push rod of the slave cylinder. Tighten the slave cylinder mounting bolts to 22 Nm (2.2 kgf/m, 1.6 lbf/ft).