## Exterior Trim

#### Front Pillar Corner Trim Replacement

20-41

1. Open the door.
2. Wrap a flat-tip screwdriver with protective tape and apply protective tape around the body to prevent damage. Carefully insert a flat-tip screwdriver next to the upper clip and detach the clip by prying on the front pillar corner trim (A). Take care not to scratch the body and related parts.

Fastener Locations

: Clip, 1

3. Close the door half-way.
4. Pull the front pillar corner trim (A) out to detach the lower clips, then remove the trim.

Fastener Locations

: Clip, 2

5. Replace any damaged clips.
6. Hold the trim up and fit the upper clip and lower clips into the holes in the body, then push on the trim until the clips snap into place.

a a a