## Fuel Supply System

#### Fuel Pulsation Damper Replacement

11-123

1. Relieve the fuel pressure (see page 11-115).

1. Remove the engine cover.

1. Remove the fuel rail mounting nuts from the fuel rail.

1. Remove the ground cable (G101).

1. Raise the fuel rail.

1. Place a wrench (A) on the fuel rail (B).

1. Place a wrench (C) on the fuel pulsation damper (D).

1. Remove the pulsation damper.

1. Install the fuel pulsation damper in the reverse order of removal with the new washers.

   NOTE:

- Replace all washers whenever the fuel pulsation damper is loosened or removed.
- If the drain hole (A) of the fuel pulsation damper cover does not face bottom, reinstall it as shown.

a a a