## Cylinder Head

#### Cylinder Head Removal (cont'd)

6-26

VTC Actuator, Exhaust Camshaft Sprocket Replacement

1. Remove the rocker arm assembly (see page 6-28).

1. Remove the cylinder head bolts. To prevent warpage, unscrew the bolts in sequence 1/3 turn at a time; repeat the sequence until all bolts are loosened.

   CYLINDER HEAD BOLTS LOOSENING SEQUENCE:

1. Remove the cylinder head.

Removal:

1. Remove the cam chain (see page 6-13).

1. Hold the camshaft with an open-end wrench, then loosen the Variable Valve Timing Control (VTC) actuator mounting bolt and exhaust camshaft sprocket mounting bolt.

1. Remove the VTC actuator and exhaust camshaft sprocket.

a a a