## Maintenance Schedule

#### Severe Conditions

3-6

Service at the indicated distance or time whichever comes first. | km x 1,000 | 7.5 | 15 | 22.5 | 30 | 37.5 | 45 | 52.5 | 60 | 67.5 | 75 | 82.5 | 90 | 97.5 | 105 | 112.5 | 120
miles x 1,000 | 4.5 | 9 | 13.5 | 18 | 22.5 | 27 | 31.5 | 36 | 40.5 | 45 | 49.5 | 54 | 58.5 | 63 | 67.5 | 72
months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
Replace engine oil |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace engine oil filter |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace air cleaner element -Use normal schedule except in dusty conditions |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Inspect valve clearance |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace fuel filter |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Drain fuel filter (water) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace timing belt | Every 150,000 km (90,000 miles) or 10 years
Inspect and replace drive belts | Inspect every 30,000 km (18,000 miles) or 2 years, replace every 150,000 km (90,000 miles) or 10 years
Replace engine coolant |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace transmission fluid |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Inspect front and rear brakes |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace brake fluid | Every 3 years
Check parking brake adjustment |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Replace pollen filter | Every 30,000 km (18,000 miles) or 1 year
Check lights alignment |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Test drive (noise, stability, dashboard operations) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Visually inspect the following items:
Tie rod ends, steering gearbox and boots |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
All fluid levels and condition of fluid
Exhaust system
Fuel lines and connections
Tyre condition

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot [over 35°C (95°F)] conditions.
- Extensive idling or long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule (see page 3-4).

a a a