## Doors

#### Front Door Glass Outer Weatherstrip Replacement

20-13

Front Door Weatherstrip Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the door.

1. Remove the power mirror/manual mirror (see page 20-33).
2. Starting at the rear, pry the door glass outer weatherstrip (A) up to detach the clips (B, C), then remove the weatherstrip.

   Fastener Locations
   B : Clip, 4 | C : Clip, 1

3. Install the weatherstrip in the reverse order of removal, and replace any damaged clips.

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. At the front pillar, remove the door stop mounting bolt (A).

   Fastener Locations
   A : Bolt, 1 | B : Clip, 1 | C: Clip, 17

2. Detach the clips (B, C), then remove the door weatherstrip (D).
3. Install the weatherstrip in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the weatherstrip is installed in the holder (D) securely.
- Apply liquid thread lock to door stop mounting bolt before installation.
- Check for water leaks (see step 7 on page 20-25).