## Interior Trim

#### Trim Removal/Installation - Door Area

20-34

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.
- LHD is shown, RHD is symmetrical.

Remove the trim as shown. To remove the door sill trim and centre-pillar upper trim, remove the side trim panel as necessary (see page 20-35).

Install the trim in the reverse order of removal and note these items:

- Replace any damaged clips.
- Before installing the anchor bolts, make sure there are no twists or kinks in the belts.

  Fastener Locations

  A : Clip, 2B : Clip, 3C : Clip, 7

  (Black)(White)

1. CENTRE PILLAR UPPER TRIM
2. To headliner
3. PIN
4. FRONT SEAT BELT UPPER ANCHOR BOLT

   7/16 - 20 UNF

   32 Nm (3.3 kgf/m, 24 lbf/ft)

5. To headliner
6. FRONT PILLAR TRIM
7. PIN
8. DOOR OPENING TRIM
9. UPPER ANCHOR COVER
10. OPENER LOCK CYLINDER

    (For some models)

11. FRONT SIDE CAP
12. KICK PANEL
13. DOOR SILL TRIM
14. FRONT SEAT BELT LOWER ANCHOR BOLTS

    7/16 - 20 UNF

    32 Nm (3.3 kgf/m, 24 lbf/ft)

15. SIDE TRIM PANEL