## Engine Assembly

#### Engine Removal

5-3

Special Tools Required Engine tilt hanger set, 07KAK-SJ40101 NOTE:

- Use fender covers to avoid damaging painted surfaces.
- To avoid damage, unplug the wiring connectors carefully while holding the connector portion.
- Mark all wiring and hoses to avoid misconnection. Also, be sure that they do not contact other wiring or hoses, or interfere with other parts.

1. Secure the hood in the wide open position (support rod in the lower hole).

1. Make sure you have the anti-theft code for the radio, then write down the frequencies for the radio's preset buttons.

1. Disconnect the battery negative terminal first, then the positive terminal.

1. Remove the battery.

1. Remove the intake manifold cover.

1. Disconnect the Intake Air Temperature (IAT) sensor connector (A) and remove the breather hose (B), then remove the air cleaner housing (C).

1. Remove the intake air duct.

a a a