## Doors

#### Rear Door Glass, Quarter Glass, and Regulator Replacement

20-19

NOTE: Put on gloves to protect your hands.

1. Raise the glass fully.
2. Remove these items:

- Door panel (see page 20-15)
- Plastic cover, as necessary (see page 20-5)
- Rod protector, for some models (see step 3 on page 20-16)

3. Carefully move the glass (A) until you can see the bolts, then remove them. Remove the glass from the regulator (B), and carefully lower the glass. Take care not to drop the glass inside the door.

   Fastener Locations
   : Bolt, 2

4. Remove the bolts (A, B) and collar (C) from the centre channel (D). Pull the upper seal (E) away as needed, and remove the screw (F). Pull the glass run channel (G) away as needed from the centre channel.

   Fastener Locations
   A : Bolt, 1 | B : Bolt, 1 | F : Screw,1

5. Move the centre channel (A) away from the quarter glass (B), and the rear door glass (C), and remove the centre channel out through the window slot. Take care not to damage the outer weatherstrip (D).