## Standards and Service Limits

#### Engine Electrical (cont'd)

2-3

Item | Measurement | Qualification | Standard or New | Service Limit
Starter for D16V1 (KG, KR, KS models) engine with M/T (VALEO) | Output |  | 1.0kW
Commutator mica depth |  | 0.50-0.90 mm (0.020-0.035 in.) | 0.2 mm (0.008 in.)
Commutator runout |  | 0.01 mm (0.004 in.) max | 0.15 mm (0.0006 in).
Brush length |  | 18 mm (0.7 in.) | 5 mm (0.2 in)
Brush spring tension |  | 15.3-19.2 N (1.56-1.96 kgf, 3.44-4.32 lbf) |

Engine Assembly

Item | Measurement | Qualification | Standard or New | Service Limit
Compression | Pressure check at 250 rpm (min-1) with wide open throttle. (See Design Specs for ratio.) | Minimum | 930 kPa (9.5 kgf/cm2, 135 psi) | -
Maximum variation | 200 kPa (2.0 kgf/cm2, 28 psi) | -