## Cylinder Head

#### Auto-Tensioner Removal/Installation (cont'd)

6-23

Chain Case Oil Seal Installation

1. Remove old liquid gasket from the chain case cover mating surfaces, bolts and bolt holes.

1. Clean and dry the chain case cover mating surfaces.

1. Apply liquid gasket, P/N 08C70-K0234M, 08C70-K0334M or 08C70-X0331S, evenly to the chain case mating surface of the chain case cover and to the inner threads of the holes.

   NOTE: Do not install the parts if 5 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue.

1. Install the chain case cover.

Special Tools Required

- Handle driver, 07749-0010000
- Driver attachment, 52 x 55 mm, 07746-0010400

1. Use the special tools to drive a new oil seal squarely into the chain case to the specified installed height.

1. Measure the distance between the chain case surface and oil seal.

Oil Seal Installed Height:

33.0 - 33.7 mm (1.30 - 1.33 in.)

a a a