## Rear Side Outer Panel

#### Removal

3-7

- Cut and pry off the rear side outer panel.
- Check the rear combination adaptor position, and check it for damage. If necessary, replace the rear combination adopter and rear gutter as an assembly.
- Check the centre pillar stiffener position and check it for damage. If necessary, cut and replace it.

  1. CENTRE PILLAR STIFFENER
  2. INNER PANEL
  3. REAR DAMPER STIFFENER
  4. PARCEL SHELF
  5. REAR COMBINATION ADAPTOR
  6. REAR GUTTER
  7. REAR PANEL
  8. REAR COMBINATION ADAPTOR
  9. OUTER PANEL
  10. REAR FLOOR
  11. SIDE SILL REINFORCEMENT