## Manual Transmission

#### Transmission Installation

13-9

1. Check the two dowel pins are installed in the clutch housing.

2. Apply Super High Temp Urea Grease (P/N 08798-9002) to the release fork (A) and the release bearing (B). Install the release fork and the release bearing.

3. Place the transmission on the transmission jack and raise it to the engine level.
4. Install the three lower transmission mounting bolts.

5. Install the clutch cover (A) and engine stiffener (B).

Steel oil pan type:

Aluminium oil pan type: