## Automatic Transmission

#### General Troubleshooting Information (cont'd)

14-7

5-door Model SRS components are located in this area. Review the SRS components locations, precautions and procedures in the SRS section before performing repairs or service.

1. Remove the screws securing the bottom of the glove box, then remove the glove box with removing the stops.
2. Remove the lower cover.
3. Remove the mounting bolts (A) on both sides of the PCM and loosen upper mounting bolt (B), then remove the PCM (C).

4. Inspect the circuit on the PCM, according to the DTC troubleshooting, with a digital multitester (A) and tapered tip probe (B) as shown.

5. If you cannot get to the wire side of the connector or the wire side is sealed, disconnect the connector and use the tester probe to probe the connectors from the terminal side. Do not force the probe into the connector.