## Keyless/Power Door Lock System

#### Super Locking Control Unit Input Test

22-234

1. Remove the each door panel (see page 20-7).
2. Disconnect the 8 P connector (A) from the super locking control unit (B).Inspect the connector and socket terminals to be sure they are all making good contact.

- If the terminals are bent, loose or corroded, repair them as necessary and recheck the system.
- If the terminals look OK, make the following input tests at the connector.

- If a test indicates a problem, find and correct the cause, then recheck the system.
- If all the input tests prove OK, the control unit must be faulty, replace it.

Driver's | Passenger's

Wire side of female terminals | Wire side of female terminals