## Doors

#### Front Door Glass and Regulator Replacement (cont'd)

20-12

Front Door Sash Trim Replacement

6. Install the glass and regulator in the reverse order of removal, and note these items:

- Roll the glass up and down to see if it moves freely without binding.
- Make sure that there is no clearance between the glass and glass run channel when the glass is closed.
- Adjust the position of the glass as necessary (see page 20-24).

NOTE: Take care not to scratch the door.

1. Turn the door weatherstrip (A) at the rear upper corner, and remove the screw.

   Fastener Location
   : Screw, 1

2. Lift up the door sash trim (B) to release the hooks (C), then remove the trim. Take care not to damage the door glass outer weatherstrip (D).
3. Install the trim in the reverse order of removal.