## Standards and Service Limits

#### CVT and Differential (cont'd)

2-19

Item | Measurement | Qualification | Standard or New | Service Limit
CVT differential carrier | Pinion shaft contact area I.D. |  | 18.010-18.028 mm (0.709-0.710 in.) | -
Carrier-to-pinion shaft clearance |  | 0.023-0.057 mm (0.001-0.002 in.) | 0.1 mm (0.004 in.)
Driveshaft contact area I.D. |  | 26.025-26.045 mm (1.0246-1.0254 in.) | -
Carrier-to-driveshaft clearance |  | 0.045-0.086 mm (0.002-0.003 in.) | 0.12 mm (0.005 in.)
Set ring-to-carrier bearing outer race clearance |  | 0-0.15 mm (0-0.006 in.) | Adjust
CVT differential pinion gear | Backlash |  | 0.08-0.15 mm (0.003-0.006 in.) | -
I.D. |  | 18.042-18.066 mm (0.7103-0.7113 in.) | -
Pinion gear-to-pinion shaft clearance |  | 0.055-0.095 mm (0.0022-0.0037 in.) | 0.15 mm (0.006 in.)

a a a