## Manual Transmission

#### Transmission Removal (cont'd)

13-7

1. Remove the three upper transmission mounting bolts.

1. Raise the vehicle and make sure it is securely supported.

1. Drain the transmission fluid. Reinstall the drain bolt using a new O-ring (see page 13-4).

1. Remove the splash shield.

1. Remove the driveshafts (see page 16-3).

1. Remove the exhaust pipe A.

1. Remove the three bolts securing the transmission rear mount.

a a a