## Exterior Lights

#### Headlight Replacement

22-114
Headlight Adjustment

1. Remove the front bumper (see page 20-104).

2. Disconnect the connectors (A) from the headlight (B).

Headlight: 60/55 W

Front Position Light: 5 W

Front Turn Signal Light: 21 W (Except KK model)

Front Turn Signal/Side Marker Light:

21/5 W (KK model)

3. Remove the 5 mounting bolts, then remove the corner upper beam (C) and headlight assembly.
4. Install in the reverse order of removal.
5. After replacement, adjust the headlights to local requirements.

CAUTION Headlights become very hot in use; do not touch them or any attaching hardware immediately after they have been turned off.

Before adjusting the headlights:

- Park the vehicle on a level surface.
- Make sure the tire pressures are correct.
- The driver or someone who weights the same should sit in the driver's seat.

Adjust the headlights to local requirements by turning the adjusters (A).