## A/T Differential

#### Component Location Index

14-226

Backlash Inspection

1. SET RING, 80 mm

   Selection, page 14-230

2. FINAL DRIVEN GEAR

   Replacement, page 14-228

3. CARRIER BEARING

   Replacement, page 14-228

4. DIFFERENTIAL CARRIER

   Backlash Inspection, page 14-226

   Replacement, page 14-227

5. ROLLER, 5 x 10 mm
6. SPEEDOMETER DRIVE GEAR
7. SNAP RING
8. CARRIER BEARING

   Replacement, page 14-228

1. Place the differential assembly on V-blocks (A) and install both axles.

2. Check the backlash of the pinion gears (B) with a dial indicator (C).

   STANDARD: 0.05-0.15 mm (0.002-0.006 in.)

3. If the backlash is out of standard, replace the differential carrier.