## Exterior Lights

#### Headlight Adjuster Switch Test

22-116

4-door:

1. Remove the driver's pocket (see page 20-76).
2. Disconnect the 5 P connector (A) from the headlight adjuster switch (B), then remove the switch.

3. Measure resistance between the No. 1 and No. 3 terminals and No. 2 and No. 3 terminals at positions 0, 1, 2, and 3 by moving the switch knob.

Between the No. 1 and No. 3 terminals:

About 4.7 k ohms

Between the No. 2 and No. 3 terminals:

Knob position | 0 | 1 | 2 | 3
Resistance [About (k ohms)] | 0.7 | 1.7 | 2.0 | 2.6

5-door:

1. Remove the driver's pocket (see page 20-216).
2. Carefully push out the headlight adjuster switch (A) from behind the dashboard.

3. Disconnect the 5P connector (B) from the switch.
4. Measure resistance between the No. 1 and No. 3 terminals and No. 1 and No. 2 terminals at positions 0, 1, 2, and 3 by moving the switch knob.

Between the No. 1 and No. 3 terminals:

About 4.7 k ohms

Between the No. 1 and No. 2 terminals:

Knob position | 0 | 1 | 2 | 3
Resistance [About (k ohms)] | 0.7 | 1.4 | 1.9 | 2.4