## Front Suspension

#### Knuckle/Hub/Wheel Bearing Replacement (cont'd)

18-14

14. Separate the hub (A) from the knuckle (B) using the special tool and a hydraulic press. Take care not to deform the splashguard. Hold onto the hub to keep it from falling when pressed clear.

1. Press

1. Press the wheel bearing inner race (A) out of the hub (B) using the special tool, a commercially available bearing separator (C) and a press.

1. Press

16. Remove the snap ring (A) and the splash guard (B) from the knuckle (C).

17. Press the wheel bearing (A) out of the knuckle (B) using the special tool and a press.

1. Press