## Intake Manifold and Exhaust System

#### Turbocharger and Exhaust Manifold Installation (cont'd)

9-7

1. Tighten the exhaust manifold fastening nuts (A). Connect the turbocharger return hose (B) with new gasket (C) and connect the oil feed pipe (D) with new gaskets (E) .

1. Install the exhaust pipe A (F) with new gasket.

1. Install the acoustic cover with specified torque.

   Tightening torque:

7.4 Nm (0.75 kgf/m, 5.4 lbf/ft)

1. Install the two bolts (B) securing the EGR pipe with gasket and install the PCV tube (B) and the air flow tube assembly (C).

1. Install the exhaust manifold cover.

1. Install the turbocharger cover.

1. Install the three bolts securing the oil level gauge pipe with new O-ring (A).

a a a