## Frame

#### Frame Repair Chart (cont'd)

20-49

p | Locating hole Ø25 (0.98) | x | For upper arm bracket centre Ø15 (0.98)
q | For trailing arm Ø13 (0.51) | y1, y2 | Locating hole Ø13 (0.51)
r | Locating hole Ø25 (0.98) | z | For upper arm Ø13 (0.51)
s | Locating hole Ø20 (0.79) | a1 | For rear lower arm centre
t | Trailing arm centre | b1 | Locating hole Ø50 (1.97)
u | Rear damper centre 73 x 68 (Slot) | c1 | Locating hole Ø20 (0.79)
v | For upper arm Ø13 (0.51) |  |
w | For trailing arm Ø23 (0.51) |  |