## Torque Converter Housing

#### Countershaft Bearing Replacement

14-191

Special Tools Required

- Adjustable bearing remover set, 07JAC-PH80000
- Handle driver, 07749-0010000
- Driver attachment, 62 x 68 mm, 07746-0010500

1. Remove the countershaft bearing with the special tool.

2. Install the ATF guide plate (A).

3. Install the new countershaft bearing (B) in the housing with the special tools.