## Cylinder Head

#### Rocker Arms and Shafts Disassembly/Reassembly

6-13

NOTE:

- Identify parts as they are removed to ensure reinstallation in original location.
- Inspect the rocker shafts and rocker arms (see page 6-15).
- The rocker arms must be installed in the same positions if reused.
- When removing or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders, springs and rocker arms on the shaft.
- Prior to reassembling, clean all the parts in solvent, dry them and apply lubricant to any contact points.

D14Z6 engine:

1. COLLAR
2. Letter "B" is stamped on the rocker arm.
3. INTAKE ROCKER ARM B
4. INTAKE ROCKER SHAFT
5. INTAKE ROCKER ARM A
6. Letter "A" is stamped on the rocker arm.
7. SPRING
8. No.1 CAMSHAFT HOLDER
9. EXHAUST ROCKER ARM A
10. Letter "A" is stamped on the rocker arm.
11. EXHAUST ROCKER SHAFT
12. Letter "B" in stamped on the rocker arm
13. SPRING
14. EXHAUST ROCKER ARM A
15. No. 5 CAMSHAFT HOLDER
16. No. 4 CAMSHAFT HOLDER
17. No. 3 CAMSHAFT HOLDER
18. No. 2 CAMSHAFT HOLDER