## Intake Manifold and Exhaust System

#### Exhaust Pipe and Muffler Replacement

9-5

NOTE: Use a new gaskets when reassembling.

D15Y5, D15Y6, D17A1, D17Z1, D17Z2 engines:

1. GASKET

   Replace.

2. MUFFLER
3. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side

4. HEATSHIELD
5. EXHAUST PIPE B
6. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side

7. GASKET

   Replace.