## Doors

#### Rear Door Glass and Regulator Replacement (cont'd)

20-158

3. Pull the glass run channel (A) away as needed. Loosen the nut (B) and remove the bolt (C) securing the rear lower channel (D).

Fastener Locations
B : Nut, 1 | C : Bolt,1

4. Pull the rear lower channel (A) forward, then remove the nut portion (B) from the door and release the channel from the glass (C) by twisting the channel.

5. Pull up the rear lower channel (A), then remove it out through the window slot.