## Manual Transmission

#### Countershaft Reassembly

13-37

Exploded View

1. REVERSE GEAR
2. SPECIAL BOLT, Replace.

   118 Nm (12 kgf/m, 87 lbf/ft)

3. BALL BEARING

   Check for wear and operation.

   Note the direction of installation.

4. 35 mm SHIM
5. 6TH GEAR
6. 5TH GEAR
7. 4TH GEAR
8. 3RD GEAR
9. 2ND GEAR
10. NEEDLE BEARING

    Check for wear and operation.

11. DISTANCE COLLAR
12. FRICTION DAMPER

    Check for wear and damage.

13. TRIPLE CONE SYNCHRO
14. SYNCHRO SPRING
15. COUNTERSHAFT
16. DISTANCE COLLAR
17. NEEDLE BEARING

    Check for wear and operation.

18. 1ST GEAR
19. TRIPLE CONE SYNCHRO
20. SYNCHRO SPRING
21. 1ST/2ND SYNCHRO HUB

a a a