## Glass

#### Rear Window Replacement (cont'd)

20-46

12. Glue the fasteners (A) to the inside face of the rear window (B) as shown. Apply primer (3MN-200, or equivalent) to the inside face of the rear window as shown. If necessary, apply primer (3M N-200, or equivalent) to the areas where the window antenna terminal base (C) will be glued, then glue the base on:

- Be sure the fasteners (and window antenna terminal base cover) line up with the alignment marks (D).
- Be careful not to touch the rear window where adhesive will be applied.

Hatched area: Apply primer here

13. Glue the upper moulding (A), side mouldings (B), and lower moulding (C) around the edge of the rear window (D):

- Glue the mouldings in the numbered sequence.
- After installing the mouldings, cut the corner edge areas (E) of the mouldings as shown.
- Be careful not to touch the rear window where adhesive will be applied.