## Exterior Lights

#### Rear Fog Lights Replacement

22-122
Brake Pedal Position Switch Test

(KG, KE, KB and KH models)

1. Remove the two screws from the rear fog light (A).

   Rear Fog Light: | 21 W

2. Disconnect the 2P connector (B) from the light.

1. Disconnect the 4P connector (A) from the brake pedal position switch (B).

2. Check for continuity between the No. 1 and No. 2 terminals.

- There should be continuity when the brake pedal is pressed.
- There should be no continuity when the brake pedal is released.

3. Check for continuity between the No. 3 and No. 4 terminals (with cruise control).

- There should be no continuity when the brake pedal is pressed.
- There should be continuity when the brake pedal is released.

4. If necessary, adjust or replace the switch, or adjust the pedal height (see page 19-5).