## Manual Transmission

#### Transmission Disassembly (cont'd)

13-17

NOTE: Place the clutch housing on two pieces of wood thick enough to keep the mainshaft from hitting the workbench.

1. Remove the detent bolts (A), springs, steel balls, back-up light switch (B) and transmission hanger (C).

2. Remove the select lever assembly.

3. Remove the shift lever assembly (A) and 8 x 10 mm dowel pins (B).

4. Remove the drain plug (A), filler plug (B), vehicle speed sensor (VSS) (C) and O-ring (D).