## Seat Belts

#### Rear Seat Belt Replacement (cont'd)

23-19

Centre Belt and Seat Belt Buckles

1. Lift the seat cushion on each side up.
2. Remove the centre anchor bolts (A), and remove the seat belt buckles (B) and centre belt (C).

With centre shoulder belt:

With centre shoulder belt:

3. Remove the right seat-back (see page 20-237).
4. Separate the seat-back frame and seat-back cover/pad (see page 20-239).
5. Remove the retractor mounting bolt (A) and the retractor bolt (B), then remove the centre belt (C) and retractor (D) from the right seat-back frame (E).