## Intake Manifold and Exhaust System

#### Exhaust Pipe and Muffler Replacement (cont'd)

9-4

NOTE: Use new gaskets and self-locking nuts when reassembling.

D16V3 engine:

1. GASKET

   Replace.

2. MUFFLER
3. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side.

4. HEAT SHIELD
5. 6 X 1.0 mm

   9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

6. EXHAUST PIPE B
7. GASKET

   Replace.

8. EXHAUST PIPE A
9. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side.

10. GASKET

    Replace.

11. SELF-LOCKING NUT

    10 x 1.25 mm

    33 Nm (3.4 kgf/m, 25 lbf/ft)

    Replace.