## Air Conditioning

#### Compressor Clutch Overhaul

21-90

1. Remove the centre nut (A) while holding the armature plate with the special tool (B).

1. B

   A/C CLUTCH HOLDER

   07NAB-HAC0100

1. Remove the armature plate (A) and shim(s) (B), taking care not to lose the shim(s). If the clutch needs adjustment, increase or decrease the number and thickness of shims as necessary, then reinstall the armature plate and recheck its clearance (see page 21-89).

3. If you are replacing the field coil, remove the snap ring (A) with snap ring pliers, then remove the rotor pulley (B). Be careful not to damage the rotor pulley and compressor.

4. Remove the bolt and holder (A), then disconnect the field coil connector (B). Loosen the clamp screw (C) to free the field coil wire. Remove the snap ring (D) with snap ring pliers, then remove the field coil (E). Be careful not to damage the field coil and compressor.