## Frame

#### Frame Repair Chart

20-272

Top view:

Unit: mm (in) Ø: Inner diameter | a | For sub-frame Ø15 (0.59) | e | Damper centre Ø78 (3.07)
| b1 | For engine mount Ø13 (0.51) | f | For damper mount Ø11.5 (0.45)
| b2 | For engine mount Ø13 (0.51) | g | For damper mount Ø11.5 (0.45)
| b3 | For engine mount Ø13 (0.51) | h | For sub-frame Ø11 (0.43)
| c1 | For transmission mount Ø13 (0.51) | i | For sub-frame Ø15 (0.59)
| c2 | For transmission mount Ø13 (0.51) | j | Locating hole Ø25 (0.98)
| c3 | For transmission mount Ø13 (0.51) | k | Locating hole Ø50 (1.97)
| d | For damper mount Ø11.5 (0.45) |  |